InS_StArT
GCS1ODI.COM
1.0
^Grey Cell Pocket Network Adaptor GCS1000,GCS1ODI.COM,IE0
?System Configuration.
!RIE0(INT)
?Note: Interrupt activity is automatically detected and configured by the PC-Zen Pocket Network Adaptor.
!RIE0(PORT)
?Note: Port address is automatically detected and configured by the PC-Zen Pocket Network Adaptor.
$OIE0(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*RIE0(FRAME) Frame Type
?Note: Ethernet_802.2 is now the default frame type for ODI Drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
