FORCEHI - Low Memory Reservation System
	  (c) Copyright 1990,  M. A. D.  Software, All Rights Reserved.
								004012
Syntax

	FORCEHI [-r] [-q] [-s] [command...]


Description

FORCEHI allows the user to lock low memory so that any drivers that are
subsequently loaded can be forced to use high memory instead of low memory.
Since low memory is a limited resource and some drivers can only be loaded
into low memory, FORCEHI can be used to force drivers that can be run out of
high memory into high memory, leaving low memory available for other drivers.

The options are:

-r	By default, FORCEHI will reserve low memory so that no other
	drivers can be loaded there.  The -r option releases any memory
	that is being held by FORCEHI.

-q	causes FORCEHI to run silently with no messages being displayed
	if everything works like it should.  Any errors will be reported.

-f	causes FORCEHI to run silently with no messages being displayed
	regardless of how successful the operation is.

command...	Will be executed as though it was the only command on the
	command line.  This command is executed after FORCEHI has
	reserved or released low memory.  If FORCEHI is unable to reserve
	or release memory (see -r option), it will not execute the command
	that was specified.  If the -f option is used, the specified command
	will always be executed regardless of whether FORCEHI is able to
	reserve or release memory successfully.


Notes

FORCEHI will not cause a driver that can only run in low memory to be usable
in high memory.

The SYSGEN command should not be used while FORCEHI has memory reserved.


Copyright Information

FORCEHI, program and documentation, Copyright 1990, by M. A. D.  Software,
All Rights Reserved and is provided on an "AS IS" basis.

The purchaser may not transfer or provide copies of the binary, object,
executable or source of this program to any third party without prior
written permission from M. A. D. Software.

