MAPMEM(U)							MAPMEM(U)
	  (C) 1990, 1991 M. A. D. Software, All Rights Reserved.

Name
	MAPMEM - Displays memory utilization.

Syntax
	MAPMEM [-demprst] [> file | device] [; command]

Description

MAPMEM produces a detailed report on memory utilization.  Each memory module
is identified and listed according to type (disk, character, other).  The
location and size information is also displayed.

By default, MAPMEM displays a summary of low and high memory, the names
and locations of memory modules that support each active logical drive, and
finally the modules that support all active character devices.  Options are
provided to reduce the amount of information displayed or alter the format.

The options are:

-d	The lengths of modules are displayed in decimal instead of hex.

-e	Only memory modules associated with character devices are displayed.

-r	Only memory modules associated with disk drivers are displayed.

-m	A summary of memory utilization is produced.

-s	Same as -m.

-p	The output is redirected to *PR.

-t	The titles are not displayed.

> filespec or devicespec
	*NIX file redirection.  By specifying a file or device, the output
	is sent to this file instead of the display.

;command
	After MAPMEM completes, the remainder of the command line is executed
	as a second command.  MAPMEM;DATE will display a memory map, then the
	date.

<SHIFT>@
	When pressed during output to the display, the output will be paused
	between sections.  Pressing any other key resumes output.  Ignored
	when output is redirected.


MAPMEM uses the file MAPMEM/TXT to provide the descriptions for each memory
module.  This file can be updated so that MAPMEM can recognize additional
memory modules.  The format of the file is:  drivername <TAB> description
An example is:
		$FD	LS-DOS Floppy disk driver
The description can be up to 35 characters long.  There can be up to 50
entries MAPMEM/TXT.  Additional information is provided in MAPMEM/TXT.


				Page  1







Files
	MAPMEM/TXT	Contains memory module descriptions

If you need more information on MAPMEM or if you want to obtain the LDOS 5.x/
version, please write to M.A.D. Software, P.O. Box 331323, Ft. Worth Texas,
76163.  Please include a Self-Addressed-Stamped-Envelope when requesting
information.
------
112101
